; Copyright (c) 2010,2011 Huawei Incorporated
; Manufacturer: Huawei Incorporated
;
; CDC ECM & NCM driver
;

[Version]
Signature="$WINDOWS NT$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider= %Mfg%
DriverVer=04/23/2012,2.6.2.3125
CatalogFile=ew_juwwanecm.cat

[Manufacturer]
%Mfg% = DeviceList,NTx86,NTamd64

[SourceDisksNames]
1 = %ew_juwwanecm.DiskName%,,,""

[SourceDisksFiles]
ew_juwwanecm.sys  = 1,,

; For Win2K
[DeviceList]
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_07&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_16&wwan
%VDFNCMDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_46&wwan
%NewNCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_76&wwan

%TDNCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C17&MI_00&wwan
%TDNCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C18&MI_00&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C1d&MI_01&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C1E&MI_03&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C1F&MI_02&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C21&MI_03&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C22&MI_02&wwan


%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&Subclass_02&Prot_07&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&Subclass_02&Prot_11&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&Subclass_02&Prot_37&wwan
%NewECMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_67&wwan

%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\COMPAT&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C06&MI_03&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C07&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C09&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0A&MI_02&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0C&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0E&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0F&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C14&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C15&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C16&MI_01&wwan

; ==================Icera Generic PIDs==================
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1444&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1445&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_144E&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_144F&MI_01&wwan

; ==================Icera VDF PIDs==================
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14AE&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14AF&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14B0&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14B1&MI_01&wwan

; ==================Balong VDF PIDs==================
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14A5&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14A6&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14A7&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14D6&MI_01&wwan

; For WinXP and later
[DeviceList.NTx86]

%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_07&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_16&wwan
%VDFNCMDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_46&wwan
%NewNCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_76&wwan

%TDNCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C17&MI_00&wwan
%TDNCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C18&MI_00&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C1d&MI_01&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C1E&MI_03&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C1F&MI_02&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C21&MI_03&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C22&MI_02&wwan


%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&Subclass_02&Prot_07&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&Subclass_02&Prot_11&wwan
%NewECMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_67&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&Subclass_02&Prot_37&wwan

%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\COMPAT&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C06&MI_03&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C07&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C09&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0A&MI_02&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0C&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0E&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0F&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C14&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C15&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C16&MI_01&wwan

; ==================Icera Generic PIDs==================
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1444&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1445&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_144E&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_144F&MI_01&wwan

; ==================Icera VDF PIDs==================
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14AE&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14AF&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14B0&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14B1&MI_01&wwan

; ==================Balong VDF PIDs==================
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14A5&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14A6&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14A7&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14D6&MI_01&wwan

; For XP and later x64
[DeviceList.NTamd64]

%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_07&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_16&wwan
%VDFNCMDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_46&wwan
%NewNCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_76&wwan

%TDNCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C17&MI_00&wwan
%TDNCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C18&MI_00&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C1d&MI_01&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C1E&MI_03&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C1F&MI_02&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C21&MI_03&wwan
%NCMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&PID_1C22&MI_02&wwan


%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&Subclass_02&Prot_07&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&Subclass_02&Prot_11&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&Subclass_02&Prot_37&wwan
%NewECMDeviceDesc% = ew_juwwanncm.ndi, USBCDCNCM\VID_12D1&Subclass_02&Prot_67&wwan

%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\COMPAT&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C06&MI_03&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C07&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C09&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0A&MI_02&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0C&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0E&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C0F&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C14&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C15&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1C16&MI_01&wwan

; ==================Icera Generic PIDs==================
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1444&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_1445&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_144E&MI_01&wwan
%ECMDeviceDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_144F&MI_01&wwan

; ==================Icera VDF PIDs==================
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14AE&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14AF&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14B0&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14B1&MI_01&wwan

; ==================Balong VDF PIDs==================
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14A5&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14A6&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14A7&MI_01&wwan
%VDFECMDesc% = ew_juwwanecm.ndi, USBCDCECM\VID_12D1&PID_14D6&MI_01&wwan

;-------------------------------------------------------------------------------
; Virtual Ethernet Adapter
;
[ew_juwwanecm.ndi]
*IfType         = 243 ; IF_TYPE_WWANPP
*MediaType      = 9; NdisMediumWirelessWan
*PhysicalMediaType = 8 ; NdisPhysicalMediumWirelessWan
EnableDhcp = 0 ; DHCP Disabled
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15 ; if you specify NCF_PHYSICAL, you must specify bustype
AddReg          = ew_juwwanecm.Reg, ParamsPromiscuous, ParamsFrameType, EcmFlag, FlowControlTimeOut
CopyFiles       = ew_juwwanecm.CopyFiles
[ew_juwwanecm.ndi.HW]
AddReg = ECM_AddReg

[ECM_AddReg]
HKR,,"Platform",0x00010001,0x1 
HKR,,"WWAN",0x00010001,0x1

[ew_juwwanecm.ndi.Services]
AddService      = %ServiceName%, 2, ew_juwwanecm.Service, ew_juwwanecm.EventLog

[ew_juwwanncm.ndi]
*IfType         = 243 ; IF_TYPE_WWANPP
*MediaType      = 9; NdisMediumWirelessWan
*PhysicalMediaType = 8 ; NdisPhysicalMediumWirelessWan
EnableDhcp = 0 ; DHCP Disabled
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15 ; if you specify NCF_PHYSICAL, you must specify bustype
AddReg          = ew_juwwanecm.Reg, ParamsPromiscuous, ParamsFrameType, NcmFlag, ParamsPacketsAccumulationTimeout, ParamsMaxNumOfDatagramsInNTB,FlowControlTimeOut
CopyFiles       = ew_juwwanecm.CopyFiles

[ew_juwwanncm.ndi.Services]
AddService      = %ServiceName%, 2, ew_juwwanecm.Service, ew_juwwanecm.EventLog

[ew_juwwanncm.ndi.HW]
AddReg = ECM_AddReg

;-----------------------------------------------------------------------------
;
[ew_juwwanecm.Reg]
HKR,    ,                         BusNumber,           0, "0"
HKR, Ndi,                         Service,             0, "huawei_wwanecm"
HKR, Ndi\Interfaces,              UpperRange,          0, "flpp4" and "flpp6"
HKR, Ndi\Interfaces,              LowerRange,          0, "ppip"

[ParamsPromiscuous]
;
;    Should the physical NIC be set to Promiscuous mode
;
HKR, Ndi\Params\Promiscuous,     ParamDesc, , %Promiscuous%
HKR, Ndi\Params\Promiscuous,     Default,  ,"0"
HKR, Ndi\Params\Promiscuous,     type, ,      enum
HKR, Ndi\Params\Promiscuous\enum,"1",  ,     %Promiscuous_Enable%
HKR, Ndi\Params\Promiscuous\enum,"0",  ,     %Promiscuous_Disable%

[ParamsFrameType]
HKR, Ndi\Params\FrameType,     ParamDesc, 0, %FrameType%
HKR, Ndi\Params\FrameType,     type,      0, enum
HKR, Ndi\Params\FrameType,     Default,   0, "0"
HKR, Ndi\Params\FrameType\enum,"1",       0, %FrameType_IP%
HKR, Ndi\Params\FrameType\enum,"0",       0, %FrameType_Ethernet%

[ParamsIsNtb32]
HKR, Ndi\Params\IsNtb32,      ParamDesc, , %IsNtb32%
HKR, Ndi\Params\IsNtb32,      Default, , "1"
HKR, Ndi\Params\IsNtb32,      type, , enum
HKR, Ndi\Params\IsNtb32\enum, "1", , "Yes"
HKR, Ndi\Params\IsNtb32\enum, "0", , "No"

[ParamsNTBInputSize]
HKR, Ndi\Params\NTBInputSize,     ParamDesc, , %NTBInputSize%
; If the following size is larger than the maximum allowed by the device, the
; maximum value is used. 0 means to use the maximum allowed value of the device.
HKR, Ndi\Params\NTBInputSize,     Default, , "0"
HKR, Ndi\Params\NTBInputSize,     type, , dword

[ParamsPacketsAccumulationTimeout]
HKR, Ndi\Params\PacketsAccumulationTimeout,     ParamDesc, , %PacketsAccumulationTimeout%
; Unit of PacketsAccumulationTimeout is usecs. Default value is 20 us.
HKR, Ndi\Params\PacketsAccumulationTimeout,     Default, , "20"
HKR, Ndi\Params\PacketsAccumulationTimeout,     type, , dword

[ParamsMaxNumOfDatagramsInNTB]
HKR, Ndi\Params\MaxNumOfDatagramsInNTB,     ParamDesc, , %MaxNumOfDatagramsInNTB%
HKR, Ndi\Params\MaxNumOfDatagramsInNTB,     Default, , "64"
HKR, Ndi\Params\MaxNumOfDatagramsInNTB,     type, , dword

[FlowControlTimeOut]
HKR, Ndi\Params\FlowControlTimeOut,     ParamDesc, , %FlowControlTimeout%
HKR, Ndi\Params\FlowControlTimeOut,     Default, , "2800"
HKR, Ndi\Params\FlowControlTimeOut,     type, , dword

[NcmFlag]
HKR, Ndi\Params\NcmFlag,     ParamDesc, , %NcmFlagDesc%
HKR, Ndi\Params\NcmFlag,     Default, , "1"
HKR, Ndi\Params\NcmFlag,     type, , dword

[EcmFlag]
HKR, Ndi\Params\NcmFlag,     ParamDesc, , %NcmFlagDesc%
HKR, Ndi\Params\NcmFlag,     Default, , "0"
HKR, Ndi\Params\NcmFlag,     type, , dword


;-----------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
ew_juwwanecm.CopyFiles = 12

[ew_juwwanecm.CopyFiles]
ew_juwwanecm.sys,,,0x6  ;COPYFLG_NOSKIP | COPYFLG_NOVERSIONCHECK
;-----------------------------------------------------------------------------
; Driver and Service Section
;

[ew_juwwanecm.Service]
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\ew_juwwanecm.sys
LoadOrderGroup  = NDIS
AddReg          = ew_juwwanecm.Service.Reg

[ew_juwwanecm.Service.Reg]
HKR, , TextModeFlags,    0x00010001, 0x0001
HKR, Parameters, DebugLevel, 0x00010001, 1
HKR, Parameters, WwanLogoTestOn, 0x00010001, 0

[ew_juwwanecm.EventLog]
AddReg = ew_juwwanecm.AddEventLog.Reg

[ew_juwwanecm.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

;
;--- ew_juwwanecm.ndi WDF Coinstaller installation ------
;
;[DestinationDirs]
;cdcecm_CoInstaller_CopyFiles = 11

;[ew_juwwanncm.ndi.CoInstallers]
;AddReg=cdcecm_CoInstaller_AddReg
;CopyFiles=cdcecm_CoInstaller_CopyFiles

;[ew_juwwanecm.ndi.CoInstallers]
;AddReg=cdcecm_CoInstaller_AddReg
;CopyFiles=cdcecm_CoInstaller_CopyFiles

;[cdcecm_CoInstaller_AddReg]
;HKR,,CoInstallers32,0x00010000, "wdfcoinstaller01009.dll,WdfCoInstaller"

;[cdcecm_CoInstaller_CopyFiles]
;wdfcoinstaller01009.dll

;[SourceDisksFiles]
;wdfcoinstaller01009.dll=1 ; make sure the number matches with SourceDisksNames

[ew_juwwanncm.ndi.Wdf]
KmdfService = %ServiceName%, cdcecm_wdfsect

[ew_juwwanecm.ndi.Wdf]
KmdfService = %ServiceName%, cdcecm_wdfsect

[cdcecm_wdfsect]
KmdfLibraryVersion = 1.9

;-----------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
Mfg = "HUAWEI"
ECMDeviceDesc = "HUAWEI Mobile Connect - Network Adapter"
NewECMDeviceDesc = "Mobile Connect - Network Adapter"
VDFECMDesc    = "Vodafone Mobile Broadband Network Adapter (Huawei)"
TDECMDeviceDesc = "HUAWEI Mobile CMCC Connect - Network Adapter"

NCMDeviceDesc = "HUAWEI Mobile Connect - Network Adapter"
NewNCMDeviceDesc = "Mobile Connect - Network Adapter"
VDFNCMDesc    = "Vodafone Mobile Broadband Network Adapter (Huawei)"
TDNCMDeviceDesc = "HUAWEI Mobile CMCC Connect - Network Adapter"

ew_juwwanecm.DiskName = "DriverCore Installation Disk"
Promiscuous = "Set the physical NIC to promiscuous mode"
Promiscuous_Disable = "Disable"
ServiceName = "huawei_wwanecm"
Promiscuous_Enable  = "Enable"
FrameType = "Frame Type in driver-device communications"
FrameType_Ethernet = "Ethernet"
FrameType_IP  = "IP"

IsNtb32 = "32bit mode"
NTBInputSize = "NTB input size"
PacketsAccumulationTimeout = "Packets Accumulation Timeout [usec]"
MaxNumOfDatagramsInNTB = "Maximum number of datagrams in NTB"
FlowControlTimeout = "Flow Control timeout interval in ms"
NcmFlagDesc = "Flag use to distinguish ncm or ecm"
